{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["公告稿"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"公告稿","index":0,"n_rows":108,"n_cols":9,"rows_kept":108,"merged":[[1,0,1,8],[2,0,2,8],[4,0,11,0],[5,1,10,1],[5,2,6,2],[7,2,9,2],[12,0,21,0],[13,1,17,1],[13,2,15,2],[16,2,17,2],[18,1,20,1],[19,2,20,2],[22,0,25,0],[22,1,25,1],[22,2,23,2],[24,2,25,2],[27,0,34,0],[27,1,32,1],[27,2,28,2],[29,2,30,2],[31,2,32,2],[33,1,34,1],[36,0,55,0],[37,1,55,1],[37,2,42,2],[43,2,48,2],[49,2,52,2],[53,2,55,2],[56,0,62,0],[56,1,58,1],[56,2,58,2],[59,1,62,1],[59,2,62,2],[63,0,68,0],[63,1,68,1],[63,2,64,2],[66,2,68,2],[69,0,72,0],[69,1,70,1],[69,2,70,2],[71,1,72,1],[74,0,103,0],[74,1,92,1],[74,2,77,2],[78,2,86,2],[78,8,81,8],[82,8,86,8],[87,2,89,2],[90,2,92,2],[93,1,103,1],[93,2,96,2],[97,2,101,2],[104,0,107,0],[104,1,107,1],[104,2,106,2]]}
["附件1"]
["《贵州省2024-2026年农机购置与应用补贴额一览表（第三批）》"]
["13大类23小类44品目104档次"]
["大类","小类","品目","档次编号","档次名称","基本配置和参数","中央补贴额(元)","是否通用类","备注"]
["一、耕整地机械","（一）耕地机械","1.开沟机",1.1,"开沟机","配套轮式拖拉机；开沟深度≥30cm",1600,"非通用类"]
[null,"（二）整地机械","2.耙（限圆盘耙、驱动耙）",2.1,"2-3m圆盘耙","2m≤作业幅宽＜3m",1200,"非通用类"]
[{"$nulls":3},2.2,"3m及以上圆盘耙","作业幅宽≥3m",1800,"非通用类"]
[null,null,"3.起垄机",3.1,"1—1.5m起垄机","1m≤工作幅宽＜1.5m",300,"非通用类"]
[{"$nulls":3},3.2,"1.5—2m起垄机","1.5m≤工作幅宽＜2m",900,"非通用类"]
[{"$nulls":3},3.3,"2—2.5m起垄机","2m≤工作幅宽＜2.5m",1800,"非通用类"]
[null,null,"4.筑埂机",4.1,"筑埂机","筑埂高度≥25cm；配套动力≥36.7kW",2600,"非通用类"]
[null,"（三）耕整地联合作业机械（可含施肥功能）","5.深松整地联合作业机",5.1,"2-2.5m深松联合整地机","2m≤作业幅宽＜2.5m",1900,"非通用类"]
["二、种植施肥机械","（四）种子播前处理和育苗机械设备","6.种子催芽机",6.1,"箱体式全自动温控喷淋式种子催芽机","功率≥4kW,箱体式,自动温控喷淋装置,生产率≥20kg/h",3900,"非通用类"]
[null,"（五）播种机械（可含施肥功能）","7.单粒（精密）播种机","7.1","4-5行高性能电驱单粒（精密）播种机","播种行数4、5行；排种器数量≥4个；单体结构质量≥110kg；排种器型式：气力式；最低作业速度≥10km/h；排种器驱动方式：电驱式；粒距/排肥量调节方式：电机控制调节；单体独立同步仿形；独立无级或多级镇压机构；配置播种作业监测终端（卫星接收机板卡类型及频电：北斗信号）",19300,"通用类"]
[{"$nulls":3},"7.2","6-10行高性能电驱单粒（精密）播种机","6行≤播种行数≤10行；排种器数量≥6个；单体结构质量≥110kg；排种器型式：气力式；最低作业速度≥10km/h；排种器驱动方式：电驱式；粒距/排肥量调节方式：电机控制调节；单体独立同步仿形；独立无级或多级镇压机构；配置播种作业监测终端（卫星接收机板卡类型及频电：北斗信号）",32700,"通用类"]
[{"$nulls":3},"7.3","11行及以上高性能电驱单粒（精密）播种机","播种行数≥11行；排种器数量≥11个；单体结构质量≥110kg；排种器型式：气力式；最低作业速度≥10km/h；排种器驱动方式：电驱式；粒距/排肥量调节方式：电机控制调节；单体独立同步仿形；独立无级或多级镇压机构；配置播种作业监测终端（卫星接收机板卡类型及频电：北斗信号）",51600,"通用类"]
[null,null,"8.根（块）茎种子播种机","8.1","2-3行根茎类种子播种机","2行≤播种行数≤3行",2000,"非通用类"]
[{"$nulls":3},"8.2","4行及以上根茎类种子播种机","播种行数≥4行",4000,"非通用类"]
[null,"（六）栽植机械","9.抛秧机",9.1,"7—9行水稻有序抛秧机","四轮乘坐式;7-9行",19600,"非通用类"]
[null,null,"10.移栽机","10.1","单行自走式移栽机(半自动取投苗)","作业行数：1行；自走式；自带动力；株距可调；取投苗方式：半自动",12000,"非通用类"]
[{"$nulls":3},"10.2","2行及以上自走式移栽机(半自动取投苗)","作业行数：2行及以上；自走式；自带动力；株距可调；取投苗方式：半自动",15000,"非通用类"]
[null,"（七）施肥机械","11.撒（抛）肥机","11.1","1m³及以上悬挂式固态肥抛撒机","料厢（肥箱）容积≥1m³；抛撒宽度≥5m",1000,"非通用类"]
["三、田间管理机械","（八）修剪防护管理机械","12.修剪机",12.1,"2Ah≤电池额定容量＜4Ah电动果树修剪机","锂电池；14.4V≤电池额定电压＜36V；2Ah≤电池额定容量＜4Ah；25mm≤最大剪切直径＜40mm。配备充电器1个、同等锂电池不少于2组，应具有安全防护功能。",150,"非通用类"]
[{"$nulls":3},12.2,"电池额定容量≥4Ah电动果树修剪机","锂电池；电池额定电压≥36V；电池额定容量≥4Ah；最大剪切直径≥40mm。配备充电器1个、同等锂电池不少于2组，应具有安全防护功能。",300,"非通用类"]
[null,null,"13.枝条切碎机",13.1,"刀辊（盘）直径50-300mm枝条切碎机","50mm≤辊（盘）直径＜300mm；刀片（锤片）数量≥2个；结构型式：盘式、鼓式；配套动力：汽油机、柴油机、电机≥4.7kW或拖拉机；切削直径≥50mm",880,"非通用类"]
[{"$nulls":3},13.2,"刀辊（盘）直径300mm及以上枝条切碎机","辊（盘）直径≥300mm；刀片（锤片）数量≥2个；结构型式：盘式、鼓式；配套动力：汽油机、柴油机、电机≥7.35kW或拖拉机；切削直径≥75mm",1200,"非通用类"]
["四、灌溉机械","（九）微灌设备","14.灌溉首部",14.1,"流量80m³/h以上灌溉首部","流量≥80m³/h；灌溉水增压设备；过滤设备；水质软化设备；灌溉施肥一体化设备；营养液消毒设备",350,"非通用类"]
["五、收获机械","（十）粮食作物收获机械","15.割晒机",15.1,"工作幅宽1m以上悬挂式割晒机","不带动力，悬挂式：作业幅宽＞1m",330,"非通用类"]
[{"$nulls":3},15.2,"工作幅宽1m以上手扶式割晒机","手扶式；作业幅宽＞1m；配套动力≥4kW",800,"非通用类"]
[null,null,"16.玉米剥皮机",16.1,"2-5对辊玉米剥皮机","2≤辊筒对数≤5",400,"非通用类"]
[{"$nulls":3},16.2,"6对辊以上玉米剥皮机","辊筒对数≥6",900,"非通用类"]
[null,null,"17 .脱粒机",17.1,"滚筒长度700mm及以下玉米脱粒机","滚筒长度≤700mm",65,"非通用类"]
[{"$nulls":3},17.2,"滚筒长度700mm以上玉米脱粒机","滚筒长度＞700mm",85,"非通用类"]
[null,"（十一）油料作物收获机械","18.大豆收获机","18.1","6kg/s及以上辅助驾驶自走履带式大豆收获机","结构型式：自走履带式，全喂入；喂入量≥6kg/s；拨禾轮型式：弹齿式;前装辅助驾驶（系统）设备",43300,"通用类"]
[null,null,"19.花生收获机","19.1","15kW及以上花生摘果机","花生摘果机；配套动力≥15kW",2900,"非通用类"]
["六、设施种植机械","（十二）食用菌生产设备","20.菌料装瓶（袋）机",20.1,"生产率2.3m³/h及以上食用菌料自动装袋机","自动套袋、装袋、扎口；生产率≥2.3m³/h",5900,"非通用类"]
["七、饲料（草）收获加工运输设备","（十三）饲料（草）收获机械","21.草捆包膜机","21.1","1.1kW及以上饲草裹包机","功率≥1.1kW，草捆直径≥500mm",1000,"非通用类"]
[null,"（十四）饲料（草）加工机械","22.铡草机","22.1","0.3-1t/h铡草机","0.3t/h≤生产率（干秸秆）＜1t/h；含动力",200,"非通用类"]
[{"$nulls":3},"22.2","1-3t/h铡草机","1t/h≤生产率（干秸秆）＜3t/h；含动力",230,"非通用类"]
[{"$nulls":3},"22.3","3-6t/h铡草机","3t/h≤生产率（干秸秆）＜6t/h；含动力",340,"非通用类"]
[{"$nulls":3},"22.4","6-10t/h铡草机","6t/h≤生产率（干秸秆）＜10t/h；含动力",610,"非通用类"]
[{"$nulls":3},"22.5","10-15t/h铡草机","10t/h≤生产率（干秸秆）＜15t/h；含动力",1050,"非通用类"]
[{"$nulls":3},"22.6","15t/h及以上铡草机","生产率（干秸秆）≥15t/h；含动力",1400,"非通用类"]
[null,null,"23.饲料（草）粉碎机","23.1","0.3-1t/h揉丝机","0.3t/h≤生产率（干秸秆）＜1t/h，0.6t/h≤生产率（青秸秆）＜2t/h；含动力",200,"非通用类"]
[{"$nulls":3},"23.2","1-3t/h揉丝机","1t/h≤生产率（干秸秆）＜3t/h，2t/h≤生产率（青秸秆）＜6t/h；含动力",230,"非通用类"]
[{"$nulls":3},"23.3","3-6t/h揉丝机","3t/h≤生产率（干秸秆）＜6t/h，6t/h≤生产率（青秸秆）＜12t/h；含动力",340,"非通用类"]
[{"$nulls":3},"23.4","6-10t/h揉丝机","6t/h≤生产率（干秸秆）＜10t/h，12t/h≤生产率（青秸秆）＜20t/h；含动力",610,"非通用类"]
[{"$nulls":3},"23.5","10-15t/h揉丝机","10t/h≤生产率（干秸秆）＜15t/h，20t/h≤生产率（青秸秆）＜30t/h；含动力",1050,"非通用类"]
[{"$nulls":3},"23.6","15t/h及以上揉丝机","生产率（干秸秆）≥15t/h，生产率（青秸秆）≥30t/h；含动力",1400,"非通用类"]
[null,null,"24.饲料混合机",24.1,"1-2m³立式饲料混合机","1m³≤混合室容积＜2m³；立式",600,"非通用类"]
[{"$nulls":3},24.2,"2m³及以上立式饲料混合机","混合室容积≥2m³；立式",800,"非通用类"]
[{"$nulls":3},24.3,"1-2m³卧式饲料混合机","1m³≤混合室容积＜2m³；卧式",1000,"非通用类"]
[{"$nulls":3},24.4,"2m³及以上卧式饲料混合机","混合室容积≥2m³；卧式",1200,"非通用类"]
[null,null,"25.全混合日粮制备机",25.1,"4-9m³饲料全混合日粮制备机","4m³≤搅拌室容积＜9m³",7500,"非通用类"]
[{"$nulls":3},25.2,"9-12m³饲料全混合日粮制备机","9m³≤搅拌室容积＜12m³",12000,"非通用类"]
[{"$nulls":3},25.3,"12m³及以上饲料全混合日粮制备机","搅拌室容积≥12m³",15000,"非通用类"]
["八、畜禽养殖机械","（十五）畜禽繁育设备","26.孵化机",26.1,"5000-10000枚孵化机","5000枚≤蛋容量＜10000枚",1500,"非通用类"]
[{"$nulls":3},26.2,"10000-50000枚孵化机","10000枚≤蛋容量＜50000枚",4500,"非通用类"]
[{"$nulls":3},26.3,"50000枚及以上孵化机","蛋容量≥50000枚",11400,"非通用类"]
[null,"（十六）饲养设备","27.喂（送）料机",27.1,"数控干湿料喂料机","装料量≥80L",820,"非通用类"]
[{"$nulls":3},27.2,"50-100m塞盘式送料机","塞盘式；50m≤送料长度<100m；含电机、料斗、驱动装置、控制装置",4000,"非通用类"]
[{"$nulls":3},27.3,"100-200m塞盘式送料机","塞盘式；100m≤送料长度＜200m；含电机、料斗、驱动装置、控制装置",6000,"非通用类"]
[{"$nulls":3},27.4,"螺旋弹簧式送料机","螺旋弹簧式；输送长度≥30m，带主机",4200,"非通用类"]
["九、畜禽养殖废弃物及病死畜禽处理设备","（十七）畜禽粪污资源化利用设备","28.清粪机",28.1,"牵引刮板式清粪机（刮板为不锈钢材质）","宽度≥2m；刮板为不锈钢材质；机架为焊接后整体热镀锌；牵引刮板式",900,"非通用类"]
[{"$nulls":3},28.2,"牵引刮板式清粪机（全不锈钢材质）","宽度≥2m；全不锈钢材质；牵引刮板式",1300,"非通用类"]
[null,null,"29.畜禽粪污固液分离机",29.1,"斜筛面积0.8m²及以上粪污固液分离机","斜筛面积≥0.8m²；结构型式：筛分（斜筛）+螺旋挤压式；配备振动电机",3200,"非通用类"]
[null,null,"30.畜禽粪便发酵处理设备",30.1,"30-50m³直立罐式畜禽粪便发酵处理机","直立罐式,30m³≤盛料容器容积＜50m³",30000,"非通用类"]
[{"$nulls":3},30.2,"50-100m³直立罐式畜禽粪便发酵处理机","直立罐式,50m³≤盛料容器容积＜100m³",40000,"非通用类"]
[{"$nulls":3},30.3,"100m³及以上直立罐式畜禽粪便发酵处理机","直立罐式,盛料容器容积≥100m³",50000,"非通用类"]
["十、水产养殖机械","（十八）投饲机械","31.投（饲）饵机",31.1,"投饲机","投饲机",270,"非通用类"]
[{"$nulls":3},31.2,"风送式投料机","送料风机≥1.5kW、每小时投饲量≥300kg、料箱容量≥300kg",1500,"非通用类"]
[null,"（十九）水质调控设备","32.增氧机",32.1,"普通型增氧机","普通型增氧机；动力：电机功率≥1.5kW",470,"非通用类"]
[null,null,"33.水质调控监控设备",33.1,"固定式（立杆式或柜式）水质调控监控设备","固定式（立杆式或柜式），数据传输方式为4G及以上，监控通道数≥4个，具有溶氧、温度、酸碱度PH测量功能",1800,"非通用类"]
["十一、粮油糖初加工机械","（二十）油料初加工机械","34.油料果（籽）脱（剥）壳机",34.1,"每小时处理量≥1000kg油茶剥壳机","生产率≥1000kg/h(鲜果),剥净率≥95%,损失率≤5%,含杂率≤5%,含自动提升、剥壳、分离、清选装置,2级及以上分级剥壳",21600,"非通用类"]
["十二、果菜茶初加工机械","（二十一）果蔬初加工机械","35.果蔬分级机",35.1,"机械鲜果分选，生产率3t/h及以上水果分级机","机械鲜果分选；生产率≥3t/h",3000,"非通用类"]
[{"$nulls":3},35.2,"光电式重量分选，分级数8-16级，生产率3t/h以下水果分级机","光电式、重量分选；8≤分级数<16；生产率<3t/h",18000,"非通用类"]
[{"$nulls":3},35.3,"光电式、重量分选，分级数8-16级，生产率3t/h及以上水果分级机","光电式、重量分选；8≤分级数＜16；生产率≥3t/h",27400,"非通用类"]
[{"$nulls":3},35.4,"光电式重量分选，分级数16级及以上，生产率5t/h及以上水果分级机","光电式、重量分选；分级数≥16；生产率≥5t/h",50000,"非通用类"]
[null,null,"36.果蔬干燥机",36.1,"容积1—5m³厢式果蔬干燥机","1m³≤有效烘干容积＜5m³；结构型式：厢式；热源装置：非燃煤型",900,"非通用类","加热室厢体采用彩钢夹芯材料；彩钢夹芯板厚度≥50mm；单片彩钢板厚度≥0.3mm；厢体填充材料采用岩棉（密度≥80kg/m³）。厢体采用钢板夹芯材料；钢板夹芯板厚度≥50mm；单片钢板厚度≥0.3mm；厢体填充材料（聚氨脂）密度≥30kg/m³，（聚苯乙烯泡沫）密度≥10kg/m³。"]
[{"$nulls":3},36.2,"容积5-20m³厢式果蔬干燥机","5m³≤有效烘干容积＜20m³；结构型式：厢式；热源装置：非燃煤型",1500,"非通用类"]
[{"$nulls":3},36.3,"容积20-40m³厢式果蔬干燥机","20m³≤有效烘干容积＜40m³；结构型式：厢式；热源装置：非燃煤型",3000,"非通用类"]
[{"$nulls":3},36.4,"容积40m³及以上厢式果蔬烘干机","有效烘干容积≥40m³；结构型式：厢式热源装置：非燃煤型",5300,"非通用类"]
[{"$nulls":3},36.5,"容积1-5m³热泵型厢式果蔬干燥机","1m³≤有效烘干容积＜5m³；结构型式：厢式；热源装置：热泵；热泵额定功率(不含电辅助加热)≥2.1kW",1100,"非通用类","厢体采用钢板夹芯材料；钢板夹芯板厚度≥50mm；单片钢板厚度≥0.3mm；烘干室墙体填充材料（聚氨脂）密度≥30kg/m³，（聚苯乙烯泡沫）密度≥10kg/m³。"]
[{"$nulls":3},36.6,"容积5-10m³热泵型厢式果蔬干燥机","5m³≤有效烘干容积＜10m³；结构型式：厢式；热源装置：热泵；热泵额定功率(不含电辅助加热)≥2.4kW",2400,"非通用类"]
[{"$nulls":3},36.7,"容积10-20m³热泵型厢式果蔬干燥机","10m³≤有效烘干容积＜20m³；结构型式：厢式；热源装置：热泵；热泵额定功率(不含电辅助加热)≥3.4kW",5600,"非通用类"]
[{"$nulls":3},36.8,"容积20-40m³热泵型厢式果蔬干燥机","20m³≤有效烘干容积＜40m³；结构型式：厢式；热源装置：热泵；热泵额定功率(不含电辅助加热)≥4.5kW",8700,"非通用类"]
[{"$nulls":3},36.9,"容积40m³及以上热泵型厢式果蔬干燥机","有效烘干容积≥40m³；结构型式：厢式；热源装置：热泵；热泵额定功率(不含电辅助加热)≥9kW",11400,"非通用类"]
[null,null,"37.青果（豆）脱壳机",37.1,"生产率300-1000kg/h青核桃剥皮自动化设备","非滚筒式，300kg/h≤生产率＜1000kg/h；含电机、自动喂料、自动卸料",600,"非通用类"]
[{"$nulls":3},37.2,"生产率1000-2000kg/h青核桃剥皮自动化设备","非滚筒式，1000kg/h≤生产率＜2000kg/h；含电机、自动喂料、自动卸料",1300,"非通用类"]
[{"$nulls":3},37.3,"生产率2000kg/h以上青核桃剥皮自动化设备","非滚筒式，生产率≥2000kg/h；含电机、自动喂料、自动卸料",1800,"非通用类"]
[null,null,"38.果蔬冷藏保鲜设备",38.1,"独立库容100m³以下简易保鲜储藏设备","库容＜100m³；含制冷机组，每立方补贴额",110,"非通用类"]
[{"$nulls":3},38.2,"独立库容100-200m³简易保鲜储藏设备","100m³≤库容＜200m³；含制冷机组，每立方补贴额",84,"非通用类"]
[{"$nulls":3},38.3,"独立库容200m³及以上简易保鲜储藏设备","库容≥200m³；含制冷机组，每立方补贴额，上限5万元",40,"非通用类"]
[null,"（二十二）茶叶初加工机械","39.茶叶杀青机",39.1,"滚筒直径30-40cm杀青机","结构型式：滚筒式；30cm≤滚筒直径＜40cm",1300,"非通用类"]
[{"$nulls":3},39.2,"滚筒直径80-100cm杀青机","含热源装置；80cm≤滚筒直径＜100cm，滚筒长度≥450cm",6400,"非通用类"]
[{"$nulls":3},39.3,"滚筒直径100cm及以上杀青机","含热源装置；滚筒直径≥100cm，滚筒长度≥600cm",10000,"非通用类"]
[{"$nulls":3},39.4,"蒸汽杀青机","振动床式；蒸汽+热风，层数：3层，首层有效摊叶面积≥3m²",43200,"非通用类"]
[null,null,"40.茶叶炒（烘）干机",40.1,"3-4锅（槽）全自动茶叶炒干机","全自动控制作业；3-4锅（槽）",3700,"非通用类"]
[{"$nulls":3},40.2,"烘干面积10m²及以上百叶式茶叶烘干机","百叶式茶叶烘干机；烘干面积≥10m²",1900,"非通用类"]
[{"$nulls":3},40.3,"有效干燥容积5m³及以上滚筒式茶叶烘干机","含热风炉；滚筒式茶叶烘干机；有效干燥容积≥5 m³",19800,"非通用类"]
[{"$nulls":3},40.4,"滚筒直径80-120cm炒制机","含热源装置；80cm≤滚筒直径＜120cm",3900,"非通用类"]
[{"$nulls":3},"40.5","滚筒直径120cm及以上炒制机","含热源装置；120cm≤滚筒直径",6000,"非通用类"]
[null,null,"41.茶叶清选机",41.1,"茶叶筛选机","茶叶筛选机",700,"非通用类"]
[null,null,"42.茶叶色选机",42.1,"执行单元数60-128个的茶叶色选机","型式：茶叶色选机；60个＜执行单元数≤128个",16000,"非通用类"]
["（十三）设施环境控制设备","（二十三）设施环境控制设备","43.加温设备",43.1,"供热量400-800MJ/H生物质燃料热风炉","400MJ/h≤供热量＜800MJ/h，燃料为生物质成型颗粒，配备送料装置、温控设备等",6300,"非通用类"]
[{"$nulls":3},43.2,"供热量800-1200MJ/h生物质燃料热风炉","800MJ/h≤供热量＜1200MJ/h，燃料为生物质成型颗粒，配备送料装置、温控设备等",8300,"非通用类"]
[{"$nulls":3},43.3,"供热量大于1200MJ/h生物质燃料热风炉","供热量≥1200MJ/h，燃料为生物质成型颗粒，配备送料装置、温控设备等",12000,"非通用类"]
[null,null,"44.湿帘降温设备",44.1,"水帘降温设备","风机功率≥1.1kW，配套水帘面积≥4m²",570,"非通用类"]